# DO228 ND Canvas
# Bea Wolf
# based on work by Joshua Davidson and Nikolai V.Chr.

io.include("do228_ND.nas");

io.include("do228_ND_drivers.nas");
canvas.NDStyles["Universal"].options.defaults.route_driver = DO228RouteDriver.new();

var NDs = [ nil ];
var ND_start = [ nil ];

var nd_display = [ nil ];

var ND = canvas.NavDisplay;

var myCockpit_switches = {
	"toggle_range": {path: "/inputs/range-nm", value:40, type:"INT"},
	"toggle_weather": {path: "/inputs/wxr", value:0, type:"BOOL"},
	"toggle_airports": {path: "/inputs/arpt", value:0, type:"BOOL"},
	"toggle_ndb": {path: "/inputs/NDB", value:0, type:"BOOL"},
	"toggle_stations": {path: "/inputs/sta", value:0, type:"BOOL"},
	"toggle_vor": {path: "/inputs/VORD", value:0, type:"BOOL"},
	"toggle_dme": {path: "/inputs/DME", value:0, type:"BOOL"},
	"toggle_cstr": {path: "/inputs/CSTR", value:0, type:"BOOL"},
	"toggle_waypoints": {path: "/inputs/wpt", value:0, type:"BOOL"},
	"toggle_position": {path: "/inputs/pos", value:0, type:"BOOL"},
	"toggle_data": {path: "/inputs/data",value:0, type:"BOOL"},
	"toggle_terrain": {path: "/inputs/terr",value:0, type:"BOOL"},
	"toggle_traffic": {path: "/inputs/tfc",value:0, type:"BOOL"},
	"toggle_centered": {path: "/inputs/nd-centered",value:0, type:"BOOL"},
	"toggle_lh_vor_adf": {path: "/input/lh-vor-adf",value:0, type:"INT"},
	"toggle_rh_vor_adf": {path: "/input/rh-vor-adf",value:0, type:"INT"},
	"toggle_display_mode": {path: "/nd/canvas-display-mode", value:"VOR", type:"STRING"},
	"toggle_display_type": {path: "/nd/display-type", value:"LCD", type:"STRING"},
	"toggle_true_north": {path: "/nd/true-north", value:0, type:"BOOL"},
	"toggle_track_heading": {path: "/trk-selected", value:0, type:"BOOL"},
	"toggle_wpt_idx": {path: "/inputs/plan-wpt-index", value: -1, type: "INT"},
	"toggle_plan_loop": {path: "/nd/plan-mode-loop", value: 0, type: "INT"},
	"toggle_weather_live": {path: "/nd/wxr-live-enabled", value: 0, type: "BOOL"},
	"toggle_chrono": {path: "/inputs/CHRONO", value: 0, type: "INT"},
	"toggle_xtrk_error": {path: "/nd/xtrk-error", value: 0, type: "BOOL"},
	"toggle_trk_line": {path: "/nd/trk-line", value: 0, type: "BOOL"},
};

var canvas_nd_base = {
	init: func(canvas_group, file = nil) {

		if (file != nil) {
			canvas.parsesvg(canvas_group, file, {"font-mapper": font_mapper});

			var svg_keys = me.getKeys();
			foreach(var key; svg_keys) {
				me[key] = canvas_group.getElementById(key);
			}
		}
		me.page = canvas_group;

		return me;
	},
	getKeys: func() {
		return [];
	},
	update: func() {
		forindex( var i; NDs ){
			if( du_status[2] == 2 ){
				NDs[ i ].page.show();
				NDs[ i ].ND.update();
				ND_start[ i ].page.hide();
			} elsif( du_status[2] == 1 ) {
				ND_start[ i ].page.show();
				NDs[ i ].page.hide();
			} else {
				ND_start[ i ].page.hide();
				NDs[ i ].page.hide();
			}
		}
		
	},
};

var canvas_ND_1 = {
	new: func(canvas_group) {
		var m = {parents: [canvas_ND_1, canvas_nd_base]};
		m.init(canvas_group);

		# here we make the ND:
		me.ND = ND.new("instrumentation/efis", myCockpit_switches, "Universal");
		me.ND.newMFD(canvas_group);
		me.ND.update();

		return m;
	},
	getKeys: func() {
		return [];
	},
	update: func() {

	},
};



var canvas_ND_1_start = {
	new: func(canvas_group, file) {
		var m = { parents: [canvas_ND_1_start , canvas_nd_base] };
		m.init(canvas_group, file);

		return m;
	},
	getKeys: func() {
		return [];
	},
	update: func() {
	}

};

setlistener("sim/signals/fdm-initialized", func {
	setprop("instrumentation/efis[0]/inputs/plan-wpt-index", -1);

	nd_display[0] = canvas.new({
		"name": "ND1",
		"size": [780, 780],
		"view": [780, 780],
		"mipmapping": 1
	});

	nd_display[0].addPlacement({"node": "efi_890r_du3"});

	NDs[ 0 ] = canvas_ND_1.new( nd_display[0].createGroup() );

	ND_start[ 0 ] = canvas_ND_1_start.new(nd_display[0].createGroup(), instrument_path~"efi-890r-start.svg");

	nd_update.start();
});

var nd_update = maketimer(0.05, func {
	canvas_nd_base.update();
});
nd_update.simulatedTime = 1;

for (i = 0; i < 2; i = i + 1 ) {
	setlistener("/instrumentation/efis["~i~"]/nd/display-mode", func(node) {
		var par = node.getParent().getParent();
		var idx = par.getIndex();
		var canvas_mode = "/instrumentation/efis["~idx~"]/nd/canvas-display-mode";
		var nd_centered = "/instrumentation/efis["~idx~"]/inputs/nd-centered";
		var mode = getprop("/instrumentation/efis["~idx~"]/nd/display-mode");
		var cvs_mode = "NAV";
		var centered = 1;
		if (mode == "ILS") {
			cvs_mode = "APP";
		}
		else if (mode == "VOR") {
			cvs_mode = "VOR";
		}
		else if (mode == "NAV"){
			cvs_mode = "MAP";
		}
		else if (mode == "ARC"){
			cvs_mode = "MAP";
			centered = 0;
		}
		else if (mode == "PLAN"){
			cvs_mode = "PLAN";
		}
		setprop(canvas_mode, cvs_mode);
		setprop(nd_centered, centered);
	});
}

setlistener("/instrumentation/efis[0]/nd/terrain-on-nd", func{
	var terr_on_hd = getprop("/instrumentation/efis[0]/nd/terrain-on-nd");
	var alpha = 1;
	if (terr_on_hd) {
		alpha = 0.5;
	}
	nd_display[0].setColorBackground(0,0,0,alpha);
});

setlistener("/flight-management/control/capture-leg", func(n) {
	var capture_leg = n.getValue();
	setprop("instrumentation/efis[0]/nd/xtrk-error", capture_leg);
	setprop("instrumentation/efis[1]/nd/xtrk-error", capture_leg);
	setprop("instrumentation/efis[0]/nd/trk-line", capture_leg);
	setprop("instrumentation/efis[1]/nd/trk-line", capture_leg);
}, 0, 0);
